ManualsContents
SettingsHelp

# sntp

Previous Next

The printer clock can be synchronized with a NTP server clock using Simple Network Time Protocol (SNTP). Use the "sntp" command to change the SNTP settings.

View settings

`msh> sntp`

NTP IPv4 server address configuration

You can specify the IPv4/IPv6 address of the NTP server.

`msh> sntp server "IPv4/IPv6_address"`

NTP hostname configuration

You can specify the hostname of the NTP server.

`msh> sntp server "hostname"`

Deleting NTP server configuration

`msh> sntp server clear`

Interval configuration

`msh> sntp interval "polling_time"`

- You can specify the interval at which the printer synchronizes with the operator-specified NTP server. The default is 60 minutes.

- The interval can be entered from 0, or between 15 and 10,080 minutes.

- If you set to "0", the printer synchronizes with the NTP server only when you turn the printer on. After that, the printer does not synchronize with the NTP server.

Time-zone configuration

`msh> sntp timezone "±hour_time"`

- You can specify the time difference between the printer clock and NTP server clock. The values are between -12:00 and +13:00.

- You can only select either the IP address or host name for the ntp server.

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search