ManualsContents
SettingsHelp

# Specifications for Auto Reverse Document Feeder (Types 3 and 4)

Previous Next

Mode:

Batch mode, SADF mode, Mixed Sizes mode, Custom Size originals mode

Original size (mainly Europe and Asia):

- One-sided originals: A3–B6 JIS, 11 × 17–81/2 × 11

- Two-sided originals: A3–A5, 11 × 17–81/2 × 11

Original size (mainly North America):

- One-sided originals: 11 × 17–51/2 × 81/2, A3–A4

- Two-sided originals: 11 × 17–51/2 × 81/2, A3–A4

Original weight:

- One-sided originals: 40–128 g/m2 (11–34 lb. Bond)

- Two-sided originals: 52–128 g/m2 (14–34 lb. Bond)

Number of originals to be set:

100 sheets (80 g/m2, 20 lb. Bond)

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search