ManualsContents
SettingsHelp

# Forwarding per Sender

Previous Next

This section describes how to specify Forwarding when registering a special sender.

You can register the fax, IP-Fax, Internet Fax, e-mail, or folder destination as a forwarding destination.

One forward destination can be registered for each special sender. To register two or more forward destinations, use group destinations. For the maximum number of destinations you can register in a group, see Maximum Values.

For details about the forwarding function, see Forwarding Received Documents.

Press [Forwarding per Sender].

Select [On] or [Off].

If you select [Off], proceed to step 6.

Specify an end receiver using the destination list, and then press [OK].

Press the transmission type tab to switch the transmission type between fax/IP-Fax, Internet Fax, e-mail, or folder.

When you specify an Internet Fax or e-mail destination as a forwarding destination, configure the settings in "Security" as necessary.

To encrypt e-mails, press [Encryption].

To attach a signature to an e-mail, press [Signature].

After configuring the settings, press [OK].

To print a Forwarding Mark on the forwarded document, press [Print Forwarding Mark] to highlight it.

Press [OK].

- Selecting [Same as Basic Settings] will result in the same setting made for "Forwarding" of "Reception File Settings" under "Reception Settings".

- For details about the "Security" setting, see Encryption and Signature for Internet Fax/E-mail.

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search