ManualsContents
SettingsHelp

# Copying onto OHP Transparencies

Previous Next

- Usually only one side of OHP transparencies can be used for printing. Be sure to load them with the print side down.

- When copying onto OHP transparencies, remove copied sheets one by one.

- The Duplex function cannot be used with OHP transparencies. If the Duplex function is specified, press [1 sided 2 sided:TtoT] to cancel the setting.

- When copying onto OHP transparencies, use A4 or 81/2 × 11 size sheets, and specify its size.

Load the paper face down in the bypass tray.

[Bypass] is automatically selected.

Press the [] key.

Press [Paper Size].

Specify the paper size, and then press [OK].

Press [Paper Type].

Press [OHP (Transparency)], and then press [OK] twice.

Place the originals, and then press the [Start] key.

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search