ManualsContents
SettingsHelp

# Routing received documents utilizing extra G3 lines

Previous Next

You can route received documents to pre-registered destinations according to the line used for reception.

To use this function, pre-registered the following settings:

For G3-1 line

- Register a Personal Box or Transfer Box with the SUB Code "1" and register a receiver or receiving station.

- Select "On" for Parameter Setting (switch 32, bit 4).

For G3-2 line

- Register a Personal Box or Transfer Box with the SUB Code "2" and register a receiver or receiving station.

- Select "On" for Parameter Setting (switch 32, bit 5).

For G3-3 line

- Register a Personal Box or Transfer Box with the SUB Code "3" and register a receiver or receiving station.

- Select "On" for Parameter Setting (switch 32, bit 6).

You can register the fax, IP-Fax, Internet Fax, e-mail, or folder destination as a routing destination.

For details about Personal Box, see Box Settings.

For details about the Parameter Settings, see Parameter Settings.

For details about the optional units required for this function, see "Functions Requiring Optional Configurations", Getting Started.

- This function is not available when you set received documents to be delivered to the network delivery server.

- When the dialed number matches the SUB Code programmed in the Personal Box, if the destinations are not programmed, this function does not work.

- Documents received through Internet Fax and IP-Fax cannot be routed.

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search