ManualsContents
SettingsHelp

# Basic Procedure for Transmissions (Memory Transmission)

Previous Next

This section describes the basic procedure for transmitting documents using Memory Transmission.

You can specify the fax, IP-Fax, Internet Fax, e-mail, or folder destinations. Multiple types of destination can be specified simultaneously.

- It is recommended that you call the receivers and confirm with them when sending important documents.

- If there is a power failure (the main power switch is turned off) or the machine is unplugged for about one hour, all the documents stored in memory are deleted. As soon as the main power switch is turned on, the Power Failure Report is printed to help you check the list of deleted files. See "Turning Off the Main Power / In the Event of Power Failure", Troubleshooting.

Press the [Home] key on the top left of the control panel, and press the [Facsimile] icon on the [Home] screen.

Make sure "Ready" appears on the screen.

Make sure [Immed. TX] is not highlighted.

Place the original into the ADF.

See Paper Specifications and Adding Paper for details.

For details about how to place originals to send using the facsimile function, see Placing Originals to Send.

Make the scan settings such as scan size and resolution.

For details about the scan settings, see Scan Settings.

Configure the transmission settings such as "TX Mode" as necessary.

Specify a destination.

You can enter the destination's number or address directly or select from the Address Book by pressing the destination key.

If you make a mistake, press the [Clear] key, and then enter again.

For details about specifying a destination, see Specifying a Destination.

When sending the same original to several destinations (broadcasting), specify the next destination.

If you send documents to Internet Fax or e-mail destinations or enable the "E-mail TX Results" function, specify a sender.

For details, see Sender Settings.

Press the [Start] key.

- If memory is full (0% appears in "Memory" at the upper right of the screen), Memory Transmission is disabled. Use Immediate Transmission instead.

- If the combined total number of programmed destinations exceeds the maximum value, only Immediate Transmission is possible.

- To send documents to Internet Fax or e-mail destinations or use the E-mail TX Results function, the sender's e-mail address must be registered in the Address Book. If the sender or the sender's e-mail address is not registered in the Address Book, register them in advance. For details about registering them, see "Registering Addresses and Users for Facsimile/Scanner Functions", Connecting the Machine/ System Settings.

- If the "Auto Specify Sender Name" function is enabled, the sender is automatically specified and you can omit the procedure for specifying a sender.

- For the maximum values of the following items, see Maximum Values:

  - Number of documents you can store in memory for Memory Transmission

  - Number of pages you can store in memory (using A4 Standard <ITU-T 1 Chart>)

  - Number of destinations you can specify per file

  - Number of destinations you can specify for all files (including files in memory)

Related topics

Sending originals using the exposure glass (Memory Transmission)
PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search