ManualsContents
SettingsHelp

# Power Connection

Previous Next

| Do not use any power sources other than those that match the specifications shown. Doing so could result in fire or electric shock.

| Do not use any frequencies other than those that match the specifications shown. Doing so could result in fire or electric shock.

| Do not use multi-socket adaptors. Doing so could result in fire or electric shock.

| Do not use extension cords. Doing so could result in fire or electric shock.

| Do not use power cords that are damaged, broken, or modified. Also, do not use power cords that have been trapped under heavy objects, pulled hard, or bent severely. Doing so could result in fire or electric shock.

| Touching the prongs of the power cable's plug with anything metallic constitutes a fire and electric shock hazard.

| The supplied power cord is for use with this machine only. Do not use it with other appliances. Doing so could result in fire or electric shock.

| It is dangerous to handle the power cord plug with wet hands. Doing so could result in electric shock.

| If the power cord is damaged and its inner wires are exposed or broken, contact your service representative for a replacement. Use of damaged power cords could result in fire or electric shock.

| Be sure to disconnect the plug from the wall outlet at least once a year. There are burn marks on the plug. The prongs on the plug are deformed. If any of the above conditions exist, do not use the plug and consult your dealer or service representative. Use of the plug could result in fire or electric shock.

| Be sure to disconnect the power cord from the wall outlet at least once a year. The power cord's inner wires are exposed, broken, etc. The power cord's coating has a crack or dent. When bending the power cord, the power turns off and on. Part of the power cord becomes hot. The power cord is damaged. If any of the above conditions exist, do not use the power cord and consult your dealer or service representative. Use of the power cord could result in fire or electric shock.

| Be sure to push the plug of the power cord fully into the wall outlet. Partially inserted plugs create an unstable connection that can result in unsafe buildup of heat.

| If this machine is not going to be used for several days or longer at a time, disconnect its power cord from the wall outlet.

| When disconnecting the power cord from the wall outlet, always pull the plug, not the cord. Pulling the cord can damage the power cord. Use of damaged power cords could result in fire or electric shock.

| Be sure to disconnect the plug from the wall outlet and clean the prongs and the area around the prongs at least once a year. Allowing dust to build up on the plug constitutes a fire hazard.

| When performing maintenance on the machine, always disconnect the power cord from the wall outlet.

- Power Source

  - (mainly Europe and Asia)

    220–240 V, 10 A, 50/60 Hz

  - (mainly North America)

    120–127 V, 12 A or more, 60 Hz

  Please be sure to connect the power cord to a power source as above.

- Voltage tolerance

  - (mainly Europe and Asia)

    Voltage must not fluctuate by more than 10%.

  - (mainly North America)

    Voltage must not fluctuate by more than +8.66% or less than -10%.

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search