ManualsContents
SettingsHelp

# Entering the path of the NetWare server directly

Previous Next

Press [Manual Entry].

Press [NCP].

Select the connection type.

Press [NDS] to specify the folder in the NDS tree.

Press [Bindery] to specify the folder on the NetWare Bindery server.

Press [Manual Entry] on the right side of the path field.

Enter the path for the folder.

If you set the connection type to [NDS], and when the NDS tree name is "tree", the name of the context including the volume is "context", the volume name is "volume", and the folder name is "folder", the path will be "\\tree\volume.context\folder".

If you set the connection type to [Bindery], and when the NetWare server name is "server", the volume name is "volume", and the folder name is "folder", the path will be "\\server\volume\folder".

Press [OK].

Enter the user name for logging in to the NDS tree or NetWare Bindery server.

Press [Manual Entry] to the right of the user name field.

If you press [NDS] for [Connection Type], enter the user name, and then enter the name of the context containing the user object. If the user name is "user" and the name of the Context is "context", the user name will be "user.context".

If a password is specified for the log in user, enter it.

Press [Manual Entry] to the right of the password field.

Press [Connection Test].

A connection test is performed to check whether the specified folder exists.

If the message `“Connection with PC has failed. Check the settings.”` appears, see "Troubleshooting When Using the Scanner Function", Troubleshooting.

Check the connection test result, and then press [Exit].

Press [OK].

- If you change the protocol after entering the path name, user name, or password, a confirmation message appears.

- To change a registered path to a destination folder, press [Edit] to the left to the destination field to display the soft keyboard, enter the correct path to the folder, and then press [OK].

- You can connect only to folders that you have the read privileges for.

- The connection test may take time.

- You may not be able to press [Connection Test] right after pressing [Cancel] during a connection test.

- Even if the connection test was successful, the machine may fail to transfer the file if you do not have write privileges for the file or there is not enough free hard disk space.

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search