ManualsContents
SettingsHelp

# Multi-Image-Layout

Previous Next

Use this function to print multiple images on the specified paper.

The number of images that can be printed on one page are as follows:

Paper size | Number of images that can be specified
--- | ---
2L (5 × 7 in) | 2, 4, 8, 9
Postcard | 2, 4
100 mm × 150 mm | 2, 4
4 × 6 in | 2, 4, 8, 9
8 × 10 in | 2, 4, 8, 9, 16, 25, 32
Letter (81/2 × 11 in) | 2, 4, 8, 9, 16, 25, 32
11 × 17 in | 2, 4, 8, 9, 16, 25, 32, 49, 64
A3 | 2, 4, 8, 9, 16, 25, 32, 49, 64
A4 | 2, 4, 8, 9, 16, 25, 32
A5 | 2, 4, 8, 9, 16
A6 | 2, 4, 8
B4 | 2, 4, 8, 9, 16, 25, 32, 36, 49
B5 | 2, 4, 8, 9, 16, 25
B6 | 2, 4, 8, 9

The number and arrangement of images that can be specified are as follows:

Number of images | Vertical images × horizontal images | Paper orientation
--- | --- | ---
2 | 2 × 1 |
4 | 2 × 2 |
8 | 4 × 2 |
9 | 3 × 3 |
16 | 4 × 4 |
25 | 5 × 5 |
32 | 8 × 4 |
36 | 6 × 6 |
49 | 7 × 7 |
64 | 8 × 8 |

- A form feed may be inserted between images depending on the digital camera in use.

- Printing in the specified way may not be possible depending on the specification for the number of images to be printed.

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search