ManualsContents
SettingsHelp

# Maximum Values

Previous Next

The following list contains the maximum value for each item.

Item | Standard | Expansion memory (Optional)
--- | --- | ---
Memory | 4 MB | 28 MB
Number of documents you can store in memory for Memory Transmission | 800 | 800
Number of received documents you can store on the machine's hard disk | 800 | 800
Number of pages you can store in memory (using A4 Standard <ITU-T 1 Chart>) | Approx. 320 | Approx. 2,240
Number of destinations you can register in the Address Book | 2,000 | 2,000
Number of groups you can register | 100 | 100
Number of destinations you can register in a group | 500 | 500
Number of forwarding destinations or number of receivers for Transfer Box that you can specify | 498 | 498
Number of destinations you can specify per file | 500 | 500
Number of destinations you can specify for all files (including files in memory) | 2000 | 2000
Number of destinations you can search at a time using [Search Dest.] | 100 | 100
Number of recent destinations the machine can store | 10 | 10
Number of digits that can be included in a destination | 128 | 128
Number of digits for a SEP/SUB/PWD/SID Code | 20 | 20
Total number of Personal Boxes, Information Boxes, and Transfer Boxes that can be programmed | 150 | 150
Number of characters you can enter in the e-mail subject line | 128 | 128
Number of communication results you can check on this machine | 200 | 200
Number of communication results printed in the Journal | 50 | 50
Number of characters that can be included in a special sender's name | 24 | 24
Number of special senders you can register | 250 | 250
Number of LAN-Fax Driver transmission results you can check using Web Image Monitor on a network computer | 70 | 70
Number of documents sent from a LAN-Fax Driver that the machine can retain as files to be sent | 800 | 800
Number of destinations you can register into a Keystroke Program | 500 | 500
Number of Keystroke Programs you can register | 100 | 100
Number of characters you can enter for a program name | 20 | 20
Number of documents you can print at a time in [Print / Delete Stored Reception File] | 30 | 30
Number of documents you can delete at a time in [Print / Delete Stored Reception File] | 30 | 30
Number of stored documents you can specify at a time in [Select Stored File] | 30 | 30
Number of stored pages you can send in one operation in [Select Stored File] | 1,000 | 1,000
Number of stored documents you can print at a time using [Print 1st Page] | 30 | 30
Number of stored documents you can print at a time using [Print File] | 30 | 30
Number of documents you can store in the Document Server using the facsimile function | 3,000 | 3,000
Number of pages per document you can store in the Document Server | 1,000 | 1,000
Number of pages you can store in the Document Server (in total - copy function, facsimile function, printer function, and scanner function) (Using ITU-T 4 Chart) | Approx. 9,000 | Approx. 9,000
Number of destinations you can register in the Address Book of the LAN-Fax | 2,000 | 2,000
Number of destinations you can specify at once using LAN-Fax | 500 | 500

- The maximum number of pages that can be stored or transmitted may decrease depending on the contents of documents.

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search