ManualsContents
SettingsHelp

# Using Pure IP in the NetWare Environment

Previous Next

Follow the procedure below to connect this machine as a print server in a pure IP environment of NetWare.

- When creating a queued print server in a pure IP environment of NetWare, create a print queue on the file server using NetWare Administrator.

- This machine is not available as a remote printer for use in a pure IP environment.

- To use the machine in a pure IP environment, set it to IPv4.

Setting up using NWadmin

From Windows, start NWadmin.

For details about NWadmin, see the NetWare manuals.

Select the object in which the print queue is located in the directory tree, and then click [Create] on the [Object] menu.

In the [Class of new object] box, click [Print Queue], and then click [OK].

In the [Print Queue Name] box, enter the name of the print queue.

In the [Print Queue Volume] box, click [Browse].

In the [Available objects] box, click the volume in which the print queue is created, and then click [OK].

Check the settings, and then click [Create].

Select the object in which the printer is located, and then click [Create] on the [Object] menu.

In the [Class of new object] box, click [Printer], and then click [OK].

In the [Printer name] box, enter the printer name.

Select the [Define additional properties] check box, and then click [Create].

Click [Assignments], and then click [Add] in the [Assignments] area.

In the [Available objects] box, click the queue you created, and then click [OK].

Click [Configuration], click [Parallel] in the [Printer type] list, and then click [Communication].

Click [Manual load] in the [Communication type] area, and then click [OK].

Check the settings, and then click [OK].

Select a context specified, and then click [Create] on the [Object] menu.

In the [Class of new object] box, click [Print Server], and then click [OK].

In the [Print Server Name] box, enter the print server name.

Use the same print server name specified using Web Image Monitor.

Select the [Define additional properties] check box, and then click [Create].

Click [Assignments], and then click [Add] in the [Assignments] area.

In the [Available objects] box, click the queue you created, and then click [OK].

Check the settings, and then click [OK].

Start the print server by entering the following from the console of the NetWare server.

If the print server is in operation, quit and restart it.

To quit

`CAREE: unload pserver`

To start

`CAREE: load pserver [print server name]`

Setting up using Web Image Monitor

Start Web Image Monitor.

Click [Login].

A dialog box for entering the login user name and login password appears.

Enter the login user name and password, and then click [Login].

For details about the login user name and password, consult your network administrator.

Depending on the configuration of your Web browser, the login user name and password might be saved. If you do not want to save them, configure your Web browser's settings so that this information is not saved.

Click [Configuration] on the [Device Management] menu.

Under "Network", click [NetWare].

For the setting items, refer to step5 of the procedure under "Configuring NetWare Settings".

Confirm the settings, and then click [OK].

Configuration is now complete. Wait several minutes before restarting Web Image Monitor.

Click [Logout].

Quit Web Image Monitor.

- If you cannot identify the printer you want to configure, check the printer name using the configuration page printed from the printer.

- If no printer names appear in the list, match the frame types of IPX/SPXs for the computer and printer. Use the [Network] dialog box of Windows to change the frame type of the computer.

- For details about Web Image Monitor, see Using Web Image Monitor.

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search