ManualsContents
SettingsHelp

# Page Separation and Length Reduction

Previous Next

If the size of a received document is longer than the paper loaded in the machine, each page of the document can be split and printed on several sheets, or reduced and printed on a single sheet.

For example, this function splits the document if the document length is 20 mm (0.8 inch) or longer than the paper used. The document is reduced if it is less than 20 mm (0.8 inch). When a document is split, an asterisk () is inserted at the split position and about 10 mm (0.4 inch) of the split area is duplicated on the top of the second sheet.

- Your service representative can customize this function with the following settings:

  - Reduction

  - Print split mark

  - Overprinting

  - Overprinting length

  - Guideline for split

- You can adjust the overprinting and reduction lengths within the following ranges:

  - Overprinting length: 4 mm (0.2 inch), 10 mm (0.4 inch), 15 mm (0.6 inch)

  - Guideline for split: 5–155 mm (5 mm steps)/0.2–6.1 inches (0.2 inch steps)

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search