ManualsContents
SettingsHelp

# Parallel Interface

Previous Next

This section describes the user tools in the Parallel Interface menu under Interface Settings.

[Parallel Interface] is displayed when this machine is installed with the IEEE 1284 interface board.

Parallel Timing

Set the timing for the control signal of the parallel interface.

Normally, you do not need to change this setting.

Default: [ACK Outside]

Parallel Communication Speed

Set the communication speed for the parallel interface. If the speed is too high, data may not be transferred smoothly. If this happens, change the setting to [Standard].

Default: [High Speed]

Selection Signal Status

Set the level for the select signal of the parallel interface.

Default: [High]

Input Prime

Set whether to validate or invalidate the input prime signal upon reception.

Normally, you do not need to change this setting.

Default: [Inactive]

Bidirectional Communication

Set the printer's response mode to a status acquisition request when using a parallel interface. If you experience problems using another manufacturer's machine, set this to [Off].

Default: [On]

When set to [Off], the bidirectional communication function will be disabled, and the printer driver will not be installed under the Windows Auto Detect function.

Signal Control

Specify how to handle errors that occur during printing operation or facsimile transmission from a computer.

Default: [Job Acceptance Priority]

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search