ManualsContents
SettingsHelp

# The applied output mode when Output Mode Switch Timer is enabled

Previous Next

If you specify a different output mode for the settings configured for receiving all documents (basic settings on the machine) or for a specific period or line (Output Mode Switch Timer), the settings which have priority differ depending on the type of output mode. For details, see the following table:

If the machine receives a fax, IP-Fax, or Internet Fax

If the following functions are specified when Output Mode Switch Timer is enabled, basic settings on the machine are enabled, not the settings of "Output Mode" in "Output Mode Switch Timer".

- Routing documents to addresses registered in Personal Boxes

- Routing e-mail received via SMTP

- Routing received documents to specified lines

- Forwarding

For details, see the following table.

Basic settings on the machine | "Output Mode" in "Output Mode Switch Timer" | Applied output mode
--- | --- | ---
"Print" | Print | Print
"Print" | Standby to Print | Standby to Print
"Print" | Forwarding | Forward documents to the address registered in Output Mode for Output Mode Switch Timer
"Print" | Store | Store
"Print" | ID Required Print | Print by entering the Print ID
Routing documents to addresses registered in Personal Boxes or routing e-mail received via SMTP | Print, Standby to Print, Forwarding, Store, or ID Required Print | Route documents to addresses registered in Personal Boxes or route e-mail received via SMTP
"Print" and routing documents to addresses registered in Personal Boxes or routing e-mail received via SMTP | Print | Route documents to addresses registered in Personal Boxes or route e-mail received via SMTP and Print
"Print" and routing documents to addresses registered in Personal Boxes or routing e-mail received via SMTP | Standby to Print, Forwarding, or Store | Route documents to addresses registered in Personal Boxes or route e-mail received via SMTP and Standby to Print
"Print" and routing documents to addresses registered in Personal Boxes or routing e-mail received via SMTP | ID Required Print | Route documents to addresses registered in Personal Boxes or route e-mail received via SMTP and Print by entering the Print ID
Routing received documents to specified lines | Print, Standby to Print, Forwarding, Store, or ID Required Print | Route received documents to specified lines
"Store" | Print, Standby to Print, Forwarding, Store, or ID Required Print | Store
"Store" and "Print" | Print | Store and Print
"Store" and "Print" | Standby to Print, Forwarding, or Store | Store and Standby to Print
"Store" and "Print" | ID Required Print | Store and Print by entering the Print ID
"Memory Lock Reception" | Print, Standby to Print, Forwarding, Store, or ID Required Print | Print by entering the Memory Lock ID
"Forwarding" | Print, Standby to Print, Forwarding, Store, or ID Required Print | Forward documents to the address registered in Reception Settings
"Forwarding" and "Print" | Print | Forward documents to the address registered in Reception Settings and Print
"Forwarding" and "Print" | Standby to Print, Forwarding, or Store | Forward documents to the address registered in Reception Settings and Standby to Print
"Forwarding" and "Print" | ID Required Print | Forward documents to the address registered in Reception Settings and Print by entering the Print ID
"Forwarding" and "Store" | Print, Standby to Print, Forwarding, Store, or ID Required Print | Forward documents to the address registered in Reception Settings and Store
"Forwarding", "Store", and "Print" | Print | Forward documents to the address registered in Reception Settings, Store and Print
"Forwarding", "Store", and "Print" | Standby to Print, Forwarding, or Store | Forward documents to the address registered in Reception Settings, Store and Standby to Print
"Forwarding", "Store", and "Print" | ID Required Print | Forward documents to the address registered in Reception Settings, Store and Print by entering the Print ID

If the machine receives an e-mail by Mail to Print or is set to automatically print reports

If reports or lists are to be printed automatically, they are also output according to the "Output Mode" setting.

"Output Mode" in "Output Mode Switch Timer" | Applied output mode
--- | ---
Print | Print
Standby to Print, Forwarding, Store | Standby to Print
ID Required Print | Print by entering the Print ID

- If the machine is set to manually print reports and lists or documents sent using the LAN-Fax Driver, all documents are printed regardless of the settings specified on "Output Mode Switch Timer".

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search