ManualsContents
SettingsHelp

# Using the machine's Address Book as the LAN-Fax destination list

Previous Next

Using SmartDeviceMonitor for Admin, you can copy the machine's Address Book data as a CSV file to a computer. This file can then be used as the LAN-Fax Destination List, and can also be installed on the machine using [Address Management Tool]. This section explains how to use the Address Book for LAN-Fax.

To use this function, you must first download SmartDeviceMonitor for Admin from the manufacturer's Web site and install it on your computer. Contact your local dealer for information on downloading SmartDeviceMonitor for Admin.

Copying the machine's Address Book to a computer

For details about operating procedure, see SmartDeviceMonitor for Admin Help.

1. Launch SmartDeviceMonitor for Admin.

   - If machine names are not displayed in the list:

     If nothing is displayed in the list, select [Search/Monitoring Settings] on the [Searched Device List] menu, specify the range of IP addresses. For example, if the range of IP addresses is 192.168.0.1–192.168.0.25, select the [Specify Address] check box, and then enter "192.168.0.1" in the [From] box and "192.168.0.25" in the [To] box. Click [Add], and then [OK].

     If the machine's IP address still does not appear in the list, check the settings of any security applications that are installed, as these settings might be disabling display of the IP address.

     You can check the machine's IP address on the control panel using "Machine IPv4 Address" on the [System Settings] menu. For details, see "Interface Settings", Connecting the Machine/ System Settings.

2. Select the model of your machine, click [Address Management Tool] on the [Tools] menu.

3. In the [Enter Authentication Information] dialog box, specify the user name and password, and then click [OK].

   Contact your administrator for the user name and password.

4. In the [Address Management Tool] dialog box, click [Export Data] on the [File] menu.

   If the `“The password information cannot be reused in any device.”` message appears, click [OK].

5. Select where to store the file, and then click [Save].

   The following three files will be stored:

   - "Machinemodel_addr.csv"

   - "Machinemodel_faxinfo.csv"

   - "Machinemodel_taginfo.csv"

   "Machinemodel_addr.csv" will be used as the Address Book file.

6. Close the [Address Management Tool] dialog box, and then close SmartDeviceMonitor for Admin.

Using the Address Book stored in the computer for LAN-Fax

Before doing the following procedure, open an existing document that you want to send and start up the LAN-Fax Driver.

For details about operating procedure, see LAN-Fax Driver Help.

1. Click the [Address Book] tab.

2. Click [Browse...].

3. Select the Address Book file, and then click [Open].

   Select "Machinemodel_addr.csv".

4. Specify the destination.

- When destinations registered in groups by this machine are inserted into Address Book, each person's destination is determined according to the following order of priority (check before inserting and changing the order of priority, if necessary): IP-Fax destination Fax number E-mail address

- Depending on the machine type, you may not be able to use the machine when it is updating the Address Book using CSV files (retrieved using SmartDeviceMonitor for Admin) that contain user codes.

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search