ManualsContents
SettingsHelp

# Original Orientation

Previous Next

When using the exposure glass, place the original face down. When using the ADF, place it face up.

Placing the original on the exposure glass

Placing the original in the ADF

When you cannot place the original as the above, you may not make copies as you want with particular functions. If this happens, change the orientation by selecting the unreadable orientation.

- Readable orientation

  Select this mode when the original orientation is the same as the copy paper orientation.

- Unreadable orientation

  Select this mode when you want to copy A3, B4 JIS, or 11 × 17 size originals. The machine rotates the copy image by 90 degrees and you can make copies as you want.

  This is useful for copying large originals with the Staple or Combine functions.

  For example, to copy A3 or 11 × 17 originals with the Combine function selected:

Press [Special Original].

Select the original orientation, and then press [OK].

- It is recommended that you use this function together with the Auto Paper Select or Auto Reduce / Enlarge function.

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search