ManualsContents
SettingsHelp

# Checking Results of LAN-Fax Transmissions

Previous Next

You can use the following methods:

Using the e-mail notification function

If a communication completes successfully, a transmission result notification e-mail is sent from the machine to a specified e-mail address.

If an error occurs during communication between your machine and a computer, or if the sent data is printed, a LAN-Fax result notification e-mail is sent to a specified e-mail address.

For details, see LAN-Fax Driver Help.

Using Web Image Monitor

You can check information about files sent using a LAN-Fax Driver.

The job history may differ from the machine's transmission results. In that case, the machine's transmission results have precedence.

For details, see Web Image Monitor Help.

- If there be any insufficient configurations of the Internet Fax or e-mail transmission on this machine, or if "Auto Specify Sender Name" is set to "Off", the E-mail TX results or LAN-Fax result notification e-mail is not transmitted, and the TX results report or LAN-Fax Result Report is printed. See "Connecting the Machine", Connecting the Machine/ System Settings for the Internet Fax settings, and see LAN-Fax Result Report for the LAN-Fax Result Report.

Related topics

LAN-Fax Result Report
PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search