ManualsContents
SettingsHelp

# Loading Orientation-Fixed Paper or Two-Sided Paper

Previous Next

Orientation-fixed (top to bottom) or two-sided paper (for example, letterhead paper, punched paper, or copied paper) might not print correctly, depending on how the originals and paper are placed.

Settings for [System Settings]

- Copier mode

  Set [Letterhead Setting] to [Yes] in [Input / Output] under the Copier / Document Server Features menu, and then place the original and paper as shown below. For details about the letterhead settings, see "Copier / Document Server Features", Copy/ Document Server.

- Printer mode

  Specify [Auto Detect] or [On (Always)] for [Letterhead Setting] under the Printer Features menu, and then place the paper as shown below. For details about the letterhead settings, see "Printer Features", Print.

Original orientation and paper orientation

The meanings of the icons are as follows:

Icon | Meaning
--- | ---
| Place or load paper scanned or printed side face up.
| Place or load paper scanned or printed side face down.

- Original orientation

  Original orientation | Exposure glass | ADF
  --- | --- | ---
  Portrait () |  |
  Landscape () | Copy Scanner |

- Paper orientation

  - Copier mode

    Copy side | Tray 1 or Tray 3 (LCT) | Trays 2–4 or the small size paper tray | Large capacity tray (LCT) | Bypass tray
    --- | --- | --- | --- | ---
    One-sided |  |  |  |
    Two-sided |  |  |  |

  - Printer mode

    Print side | Tray 1 or Tray 3 (LCT) | Trays 2–4 or the small size paper tray | Large capacity tray (LCT) | Bypass tray
    --- | --- | --- | --- | ---
    One-sided |  |  |  |
    Two-sided |  |  |  |

- In printer mode:

  - To print on letterhead paper when [Letterhead Setting] is set to [Auto Detect], you must specify [Letterhead] as the paper type in the printer driver's settings.

  - If a print job is changed partway through printing from one-sided to two-sided printing, one-sided output after the first copy may print facing a different direction. To ensure all paper is output facing the same direction, specify different input trays for one-sided and two-sided printing. Note also that two-sided printing must be disabled for the tray specified for one-sided printing.

  - For details about how to make two-sided prints, see "Printing on Both Sides of Sheets", Print.

- In copier mode:

  - For details about how to make two-sided copies, see "Duplex Copying", Copy/ Document Server.

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search