ManualsContents
SettingsHelp

# Basic Operating Procedure of WSD Scanner (Push Type)

Previous Next

- If the message `“Updating the destination list has failed. Try again?”` appears, press [OK]. The destination list will then be updated.

Press the [Home] key on the top left of the control panel, and press the [Scanner] icon on the [Home] screen.

Make sure that no previous settings remain.

If a previous setting remains, press the [Reset] key.

Press [Swtch Dest.List] to select [WSD], and then press the [OK].

If [Swtch Dest.List] is not displayed, press [WSD Dest.].

Place originals.

If necessary, specify the scan settings according to the original to be scanned.

These include the [Erase Border], adjusting image, and [Original Feed Type] settings under [Scan Settings]. For details, see Various Scan Settings.

Specify other scan conditions using the client computer. See Changing a Scan Profile.

Specify the destination.

For details, see Specifying the Destination Client Computer.

Press the [Start] key.

- You cannot preview scanned images. After pressing the [Start] key, you can view the scanned images on your computer.

- After you press the [Start] key, the client computer might time out and display the error message "Automatic Scanning could not be completed". The cause of this message is likely to be one of the following:

  - Scan processing is taking a long time.

    The machine will send the scan files again; please wait. Depending on the client computer's settings, you might have to perform a procedure on the client computer directly.

  - The operating system might not support WSD (Push Type) features.

    If the message appears every time you scan an original, it is possible that WSD (Push Type) features cannot be used. Use WSD (Pull Type) for scanning.

- To cancel scanning, press the [Stop] key. You cannot cancel scanning from a client computer.

- You cannot use WSD to send files stored on the machine.

- You cannot scan originals while other originals are being scanned.

- Two-sided originals are scanned for sideways opening (top-to-top orientation).

- If scanning does not begin after you press the [Start] key, the machine might not be registered to the computer or the profile might be incorrectly configured. For details, see Registering the machine to a client computer or Creating a New Scan Profile.

- After scan files are sent, their destination settings are automatically cleared. If you want to preserve this information, contact your local dealer for details.

- You cannot switch the screen while e-mail or other destinations are being specified. To clear the specified destination, display the destination in the destination field of each screen, and then press the [Stop] key.

Related topics

Specifying the Destination Client Computer
PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search