ManualsContents
SettingsHelp

# Interface Settings

Previous Next

Some of the settings under [Interface Settings] in [System Settings] on the control panel can be specified using Web Image Monitor and telnet.

Network
Control panel | Web Image Monitor | telnet
--- | --- | ---
[Machine IPv4 Address] [Auto-Obtain (DHCP)] | Available | Available
[Machine IPv4 Address] [Specify] "Machine IPv4 Address" | Available | Available
[Machine IPv4 Address] [Specify] "Subnet Mask" | Available | Available
[IPv4 Gateway Address] | Available | Available
[Machine IPv6 Address] "Manual Configuration Address" | Available | Available
[IPv6 Gateway Address] | Available | Available
[IPv6 Stateless Address Autoconfiguration] | Available | Available
[DNS Configuration] [Auto-Obtain (DHCP)] | Available | Available
[DNS Configuration] [Specify] "DNS Server 1-3" | Available | Available
[DDNS Configuration] | Available | Available
[IPsec] | Available | Available
[DHCPv6 Configuration] | Available | Available
[Domain Name] [Auto-Obtain (DHCP)] | Available | Available
[Domain Name] [Specify] "Domain Name" | Available | Available
[WINS Configuration] [On] "Primary WINS Server" | Available | Available
[WINS Configuration] [On] "Secondary WINS Server" | Available | Available
[WINS Configuration] [On] "Scope ID" | Available | Available
[WINS Configuration] [Off] | Available | Available
[Effective Protocol] "IPv4" | Available | Available
[Effective Protocol] "IPv6" | Available | Available
[Effective Protocol] "SMB" | Available | Available
[Effective Protocol] "NetWare" | Available | Available
[NCP Delivery Protocol] [IPX Priority] | Available | Available
[NCP Delivery Protocol] [TCP / IP Priority] | Available | Unavailable
[NCP Delivery Protocol] [IPX Only] | Available | Unavailable
[NCP Delivery Protocol] [TCP / IP Only] | Available | Unavailable
[NW Frame Type] [Auto Select] | Available | Unavailable
[NW Frame Type] [Ethernet II] | Available | Available
[NW Frame Type] [Ethernet 802.2] | Available | Available
[NW Frame Type] [Ethernet 802.3] | Available | Available
[NW Frame Type] [Ethernet SNAP] | Available | Available
[SMB Computer Name] | Available | Available
[SMB Work Group] | Available | Available
[Ethernet Speed] | Available | Available
[LAN Type] [Ethernet] | Available | Available
[LAN Type] [Wireless LAN] | Available | Available
[Ping Command] | Unavailable | Unavailable
[Permit SNMPv3 Communication] [Encryption Only] | Available | Available
[Permit SNMPv3 Communication] [Encryption / Cleartext] | Available | Available
[Permit SSL / TLS Communication] [Ciphertext Only] | Available | Unavailable
[Permit SSL / TLS Communication] [Ciphertext Priority] | Available | Unavailable
[Permit SSL / TLS Communication] [Ciphertext / Cleartext] | Available | Unavailable
[Host Name] | Available | Available
[Machine Name] | Available | Available
[IEEE 802.1X Authentication for Ethernet] | Available | Available

Wireless LAN
Control panel | Web Image Monitor | telnet
--- | --- | ---
[Communication Mode] [802.11 Ad-hoc Mode] | Available | Available
[Communication Mode] [Infrastructure Mode] | Available | Available
[SSID Setting] | Available | Available
[Ad-hoc Channel] | Available | Available
[Security Method] | Available | Available

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search