ManualsContents
SettingsHelp

# Viewing Fax Information Using Web Image Monitor

Previous Next

This section describes how to manage the machine's Address Book and documents received and stored on the machine's hard disk using Web Image Monitor on a network computer.

- It is recommended that you use Web Image Monitor running under the same network environment as this machine. Otherwise, the Web browser may not open and an error may occur.

- When entering an IPv4 address, do not begin segments with zeros. For example: If the address is "192.168.001.010", you must enter it as "192.168.1.10" to connect to the machine.

- You need to set "Store" to "On" in the Facsimile Features menu. For details about Store, see Reception File Settings.

- For details about using Web Image Monitor, see "Monitoring and Configuring the Machine", Connecting the Machine/ System Settings.

Related topics

Viewing, Printing, and Deleting Received Fax Documents Using Web Image Monitor
Registering Internet Fax Destination Information Using Web Image Monitor
PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search