ManualsContents
SettingsHelp

# PS Menu

Previous Next

This menu appears only when an optional PostScript 3 unit is installed.

Job Timeout

You can specify how long the printer waits (in seconds) before canceling the current job when the job is interrupted while being processed.

Default: [Use Driver / Command]

If you select [Use Machine Settings], enter a value between 0 and 999.

Default: "0"

When set to "0", the current job will not be canceled when interrupted.

Wait Timeout

You can specify how long the printer waits (in seconds) before it cancels receiving the job when the printer cannot detect the end of the job.

Default: [Use Driver / Command]

If you select [Use Machine Settings], enter a value between 0 and 999.

Default: "300"

When set to "0", the print job will not be canceled when the end of the job cannot be detected.

Swtchng. btwn. 1&2 Sided Prt. Func.

Select which side of paper to print on when the PS command is used to perform duplex printing, and the "setpagedevice" command is entered.

- Active

  Cancels duplex printing, and prints pages after the "setpagedevice" command has been entered on the front side of paper.

- Inactive

  Retains duplex printing, and prints pages after the "setpagedevice" command has been entered on the back side of paper.

Default: [Active]

Data Format

You can select a data format.

Default: [TBCP]

This setting is not effective when operating the machine with a parallel connection.

When operating the machine with a parallel connection, and also if the binary data is sent from the printer driver, the print job is canceled.

Resolution

You can set the print resolution in dots per inch.

Default: [600 dpi (Fast)]

Toner Saving

Reduces toner consumption when printing. When this setting is enabled, print quality may be degraded.

Default: [Off]

Colour Setting

You can make an RGB setting.

Default: [Super Fine]

Colour Profile

You can set the color profile.

Default: [Auto]

Process Colour Model

Specify the color model.

Default: [Colour]

Orientation Auto Detect

Specify whether or not to automatically detect the print data orientation.

Default: [On]

Grey Reproduction

You can specify how to print black or gray tones.

- Black/Grey by K (Black)

- Black by K (Black)

- CMY + K

- Black/Grey by K-Text Only

- Black by K (Black)-Text Only

Default: [Black/Grey by K (Black)]

- For details about how to change the Printer Features, see "Accessing User Tools", Connecting the Machine/ System Settings.

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search