ManualsContents
SettingsHelp

# Specifications for Booklet Finisher SR3100

Previous Next

Paper size for the finisher upper tray:

A3, B4 JIS, A4, B5 JIS, A5, B6 JIS, A6,

12 × 18, 11 × 17, 11 × 15, 10 × 14, 81/2 × 14, 81/2 × 13, 81/2 × 11, 81/4 × 14, 81/4 × 13, 8 × 13, 8 × 10, 51/2 × 81/2, 71/4 × 101/2,

8K, 16K, custom size

Paper weight for the finisher upper tray:

52–105 g/m2 (14–28 lb. Bond)

Stack capacity for the finisher upper tray (80 g/m2, 20 lb. Bond):

- 100 sheets: A4, 81/2 × 11 or smaller

- 50 sheets: B4 JIS, 81/2 × 14 or larger

Paper size for the finisher shift tray:

A3, B4 JIS, A4, B5 JIS,

12 × 18, 11 × 17, 11 × 15, 10 × 14, 81/2 × 14, 81/2 × 13, 81/2 × 11, 81/4 × 14, 81/4 × 13, 8 × 13, 8 × 10, 51/2 × 81/2, 71/4 × 101/2,

8K, 16K, custom size

Paper weight for the finisher shift tray:

52–256 g/m2 (14 lb. Bond–140 lb. Index)

Paper sizes that can be shifted when delivered to the finisher shift tray:

- Standard size:

  A3, A4, B4 JIS, B5 JIS, 12 × 18, 11 × 17, 11 × 15, 10 × 14, 81/2 × 14, 81/2 × 13, 81/2 × 11, 81/4 × 14, 81/4 × 13,

  8 × 13, 8 × 10, 71/4 × 101/2, 8K, 16K

- Custom size:

  Vertical: 148.0–305.0 mm (5.83–12.00 inches)

  Horizontal: 148.0–457.2 mm (5.83–18.00 inches)

  In printer or facsimile mode, the maximum horizontal length of the custom size is 460.0 mm (18.11 inches).

Paper weight that can be shifted when delivered to the finisher shift tray:

60–105 g/m2 (16–28 lb. Bond)

Stack capacity for the finisher shift tray (80 g/m2, 20 lb. Bond):

- 1,000 sheets: A4, 81/2 × 11 or smaller

- 500 sheets: B4 JIS, 81/2 × 14 or larger

Staple paper size:

A3, B4 JIS, A4, B5 JIS,

11 × 17, 11 × 15, 10 × 14, 81/2 × 14, 81/2 × 11, 71/4 × 101/2, 8 × 13, 81/2 × 13, 81/4 × 14, 81/4 × 13, 8 × 10,

8K, 16K

Staple paper weight:

64–90 g/m2 (17–24 lb. Bond)

Staple capacity (90 g/m2, 24 lb. Bond):

- Without Mixed Size:

  - 30 sheets: A3, B4 JIS, 11 × 17, 81/2 × 14, 8 × 13, 81/2 × 13, 81/4 × 14, 81/4 × 13, 11 × 15, 10 × 14, 8K

  - 50 sheets: A4, B5 JIS, 81/2 × 11, 8 × 10, 71/4 × 101/2, 16K

- With Mixed Size: 22 sheets (A3/A4, B4 JIS/B5 JIS, 11 × 17/81/2 × 11)

Stack capacity after stapling (80 g/m2, 20 lb. Bond):

- 2–9 sheets: 100 sets (A4, 81/2 × 11)

- 10–50 sheets: 100–20 sets (A4, 81/2 × 11)

- 2–9 sheets: 100 sets (A4, B5 JIS, 81/2 × 11)

- 10–50 sheets: 50–10 sets (A4, B5 JIS, 81/2 × 11)

- 2–9 sheets: 50 sets (A3, B4 JIS, 11 × 17, 81/2 × 14)

- 10–30 sheets: 50–10 sets (A3, B4 JIS, 11 × 17, 81/2 × 14)

Staple position:

3 positions (Top, Bottom, 2 Staples)

Saddle stitch paper size:

A3, B4 JIS, A4, B5 JIS, 11 × 17, 81/2 × 14, 81/2 × 11

Saddle stitch paper weight:

64–90 g/m2 (17–24 lb. Bond)

Saddle stitch capacity (80 g/m2, 20 lb. Bond):

1 set (10 sheets)

Stack capacity after saddle stitching (80 g/m2, 20 lb. Bond):

- 2–5 sheets: approx. 20 sets

- 6–10 sheets: approx. 10 sets

Saddle stitch position:

Center 2 positions

Power consumption:

60 W or less (Power is supplied from the main unit.)

Dimensions (W × D × H):

535 × 600 × 930 mm (21.1 × 23.7 × 36.7 inches)

Weight:

- Approx. 48 kg (105.9 lb.) (without punch unit)

- Approx. 50 kg (110.3 lb.) (with punch unit)

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search