ManualsContents
SettingsHelp

# Double Copies

Previous Next

One original image is copied twice on one sheet.

- You cannot use the bypass tray with this function.

- The following original size cannot be detected properly on the exposure glass:

  - (mainly Europe and Asia)

    - Types 1 and 2

      A5, 11 × 17, 81/2 × 11

    - Types 3 and 4

      A5, B6 JIS, 11 × 17, 81/2 × 11

  - (mainly North America)

    51/2 × 81/2, 10 × 14, 71/4 × 101/2, A3, A4

- If your originals are one of the above sizes, be sure to manually select the copy paper or place the originals in the ADF.

See the following table for original and copy paper sizes when using a 100% ratio:

Original size and orientation | Copy paper size and orientation
--- | ---
A5 | A4
B6 JIS* | B5 JIS
A4 | A3
A5 | A4
B5 JIS | B4 JIS
B6 JIS* | B5 JIS
51/2 × 81/2 | 81/2 × 11
51/2 × 81/2 | 81/2 × 11
81/2 × 11 | 11 × 17

* This size of original is available only with Types 3 and 4.

Press [Edit / Colour].

Press [Edit Image].

Press [Double Copies].

Press [OK].

Select the paper size.

- You can change the settings for Double Copies under [Edit] in User Tools. For details, see Edit.

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search