ManualsContents
SettingsHelp

# Stamp Text

Previous Next

This section describes the user tools in the Stamp Text menu under [Stamp].

Font

You can select the font in Stamp Text mode.

Default: [Font 1]

Size

You can select the stamp text size.

Default: [Auto]

Superimpose

You can have the stamp text printed in white when it overlaps black parts of the image.

Default: [Off]

Stamp Colour

Select the priority color when printing the text.

Default: [Black]

Stamp Setting

Specify how stamp text is printed.

- Stamp Position

  Specify where to print the Stamp Text. For details about the stamp position, see Stamps.

  Default: [Top Right]

- Adjust Stamp Position

  You can adjust the position in which the stamp is printed.

  The position where the stamp is printed and the range within which that position can be adjusted are shown in the following table. The values for defaults and possible ranges given in the table are the distance from each side of the paper.

  (mainly Europe and Asia)

  Stamp positions | Default | Possible range
  --- | --- | ---
  Top Left | 32 mm from the left edge 8 mm from the top edge | From 4 to 144 mm from the left edge From 4 to 144 mm from the top edge
  Top Centre | Center 8 mm from the top edge | From 0 to 72 mm to the right or left of the center From 4 to 144 mm from the top edge
  Top Right | 12mm from the right edge 8 mm from the top edge | From 4 to 144 mm from the right edge From 4 to 144 mm from the top edge
  Bottom Left | 32 mm from the left edge 8 mm from the bottom edge | From 4 to 144 mm from the left edge From 4 to 144 mm from the bottom edge
  Bottom Centre | Center 8 mm from the bottom edge | From 0 to 72 mm to the right or left of the center From 4 to 144 mm from the bottom edge
  Bottom Right | 12mm from the right edge 8 mm from the bottom edge | From 4 to 144 mm from the right edge From 4 to 144 mm from the bottom edge

  (mainly North America)

  Stamp positions | Default | Possible range
  --- | --- | ---
  Top Left | 1.3 inches from the left edge 0.3 inches from the top edge | From 0.1 to 5.7 inches from the left edge From 0.1 to 5.7 inches from the top edge
  Top Center | Center 0.3 inches from the top edge | From 0 to 2.8 inches to the right or left of the center From 0.1 to 5.7 inches from the top edge
  Top Right | 0.5 inches from the right edge 0.3 inches from the top edge | From 0.1 to 5.7 inches from the right edge From 0.1 to 5.7 inches from the top edge
  Bottom Left | 1.3 inches from the left edge 0.3 inches from the bottom edge | From 0.1 to 5.7 inches from the left edge From 0.1 to 5.7 inches from the bottom edge
  Bottom Center | Center 0.3 inches from the bottom edge | From 0 to 2.8 inches to the right or left of the center From 0.1 to 5.7 inches from the bottom edge
  Bottom Right | 0.5 inches from the right edge 0.3 inches from the bottom edge | From 0.1 to 5.7 inches from the right edge From 0.1 to 5.7 inches from the bottom edge

- Page to Stamp

  You can have the stamp printed on the first page or all pages.

  Default: [All Pages]

Change Job Serial No. for First Job

You can select whether or not to print the serial number after the stamped text. For details about how to specify the setting, see Printing text and serial numbers.

Default: [Off]

- For details about how to change the Copier / Document Server Features, see "Changing Default Settings", Connecting the Machine/ System Settings.

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search